CONTROL OF RE-EXPORTS OF SUPPLIES AND SERVICES [ S.L.117.06 1
SUBSIDIARY LEGISLATION 117.06
CONTROL OF RE-EXPORTS OF SUPPLIES AND 
SERVICES REGULATIONS
28th March, 1956
GOVERNMENT NOTICE 180 of 1956, as amended by Government
Notices 389 and 784 of 1957; Legal Notices 25 of 1959 and 13 of 1961.
Title.
Supplies and Services Regulations.
Prohibition.
First Schedule which are in the course of shipment on a through bill
of lading or otherwise - 
( a ) from any country specified in the Second Schedule; or
( b ) from any other country if the Comptroller of Customs
is satisfied that a person who is resident in any country
specified in the Second Schedule has acted as a
principal in the consignment of the goods,
to any country specified in the Third Schedule is prohibited unless
the goods are accompanied by a valid transit authorisation
certificate issued by the appropriate authority of the country from
which the goods were originally exported, in the form of the Fourth
Schedule.
Description of 
goods.
Cap. 37.
3. The importer of any goods referred to in regulation 2 or his
agent, shall, before transhipment, in making due entry of the goods
in terms of the Customs Ordinance and of the regulations made
thereunder, describe such goods in accordance with their
designation in the First Schedule, giving the relative quantity and/
or unit of measure or weight and deliver to the Comptroller of
Customs the aforesaid transit authorisation certificate.
Valid transit 
authorisation 
certificate.
4. No master or person in charge of a vessel shall receive on
board in the course of transhipment any goods referred to in
regulation 2 unless they are accompanied by a valid transit
authorisation certificate in the form of the Fourth Schedule.
Offences and 
penalties.
5. (1) Any person failing to comply with any of these
Regulations shall be guilty of an offence.
(2) Any person alleged to have committed an offence in sub-
regulation (1) shall be tried by the Court of Magistrates (Malta) or
the Court of Magistrates (Gozo), and shall on conviction be liable
to imprisonment for a period not exceeding six months or to a fine
( multa ) not exceeding five hundred liri, or to both such
imprisonment and fine.
(3) When any person is convicted of an offence under sub-
regulation (1), the court shall order the forfeiture of the goods to
which the offence relates, whether or not the owner thereof is a
party to the proceedings.
2 [ S.L.117.06 CONTROL OF RE-EXPORTS OF SUPPLIES AND SERVICES
Amended by:
G.N. 389 of 1957;   FIRST SCHEDULE
G.N. 784 of 1957;  (Regulation 2)
L.N. 25 of 1959.
Substituted by: PART I 
L.N. 13 of 1961.
Group 1
Aircraft, Arms and Military Stores and Appliances
Aircraft and helicopters, of the piloted or pilotless types; aero-engines and aircraft
equipment; associated equipment and components.
Arms, missiles and munitions; components and parts specially designed therefor. 
Articles (including vehicles) specially designed or adapted for military use, and all
components and parts specially designed therefor.
Biological and chemical materials adapted for use in war to produce casualties in
men or animals, or to damage crops; equipment specially designed and intended -
( a ) for their dissemination; or 
( b ) for defence against them;
components and parts specially designed therefor.
Cables, electric, buoyant types, suitable for sweeping magnetic mines.
Explosives as defined in article 2 of the Explosives Ordinance.
Ground and airborne equipment developed solely or of a kind used mainly for
aircraft, other than types in normal civil use.
Machinery and machine tools and apparatus specially designed or adapted for the
production, testing, research into and development of any of the items specified in
this Group.
Pressurized breathing equipment and partial pressure suits for use in aircraft; anti-
g suits; flak suits; parachutes of a kind used for combat personnel, cargo-dropping
and aircraft deceleration; liquid oxygen converters of a kind used for aircraft and
missiles; catapults and cartridge actuated devices of a kind utilised in emergency
escape of personnel from aircraft.
Self-contained diving and underwater swimming apparatus, the following -
Closed and semi-closed circuit (rebreathing) apparatus.
Specially designed components for use in the conversion of open-circuit
apparatus to military use.
Articles specially designed for military use with self-contained diving
and underwater swimming apparatus.
Telemetering and telecontrol equipment suitable for use with aircraft (piloted or
pilotless) and missiles (guided or unguided).
Vessels of war and propulsion machinery for such vessels; components, parts
accessories and attachments specially designed therefor.
Group 2
Atomic Energy Materials and Appliances
Centrifuges and centrifuge bowls, the following -
Centrifuges, capable of the enrichment or separation of isotopes, with
CONTROL OF RE-EXPORTS OF SUPPLIES AND SERVICES [ S.L.117.06 3
peripheral speed of 1,000 feet (305 metres) per second or more, wholly
made of, or lined with, aluminium, nickel or alloy containing 60 per
cent, or more of nickel.
Bowls for centrifuges, capable of the enrichment or separation of
isotopes, made of aluminium, nickel or alloy containing 60 per cent or
more, of nickel.
Compressors and blowers (turbo, centrifugal and axial flow types), wholly made
of, or lined with, aluminium, nickel or alloy containing 60 per cent, or more, of
nickel, having a capacity of 60 cubic feet per minute or greater.
Deuterium, heavy water, heavy parans and other compounds in which the ratio by
number of deuterium atoms to hydrogen atoms exceeds 1 to 5,000; mixtures and
solutions of any of the foregoing.
Dosimeters capable of measuring dosages above 5 roentgens, other than those
specially designed for use with medical radiation equipment.
Electrolytic cells for the production of fluorine.
Equipment specifically designed for the separation of isotopes of uranium or
lithium or of uranium and lithium.
Fissionable material, the following: 
Plutonium. 
Uranium enriched in the isotope 235. 
The isotope 233 of uranium.
Alloys, compounds or mixtures of any of the foregoing.
Furnaces, vacuum, induction type, designed to operate at pressures lower than 0.1
millimetre of mercury and at temperatures higher than 1,100º Centigrade.
Graphite; artificial, having a boron content of one part per million or less, and a
total thermal neutron absorption microscopic cross-section of 5 millibars or less per
atom, in the form of blocks, bricks, plates, rods or electrodes, from which a cube of 2
inches side or greater can be cut.
Heat exchangers (tubular) and components therefor (other than aluminium tubing)
designed to operate at pressures of 300 pounds per square inch and above and with
flow contact surfaces made of any of the following materials: 
Aluminium.
Nickel. 
Alloy containing 60 per cent or more of nickel. 
Titanium.
Zirconium.
Mass spectrographs and mass spectrometers, the following:
Mass spectrographs and mass spectrometers with analyser assemblies
capable of handling uranium hexafluoride.
Solid source mass spectrographs and mass spectrometers of high
sensitivity.
Nuclear reactors.
Positive ion sources suitable for use in mass spectrographs or mass spectrometers
and capable of handling uranium hexafluoride.
4 [ S.L.117.06 CONTROL OF RE-EXPORTS OF SUPPLIES AND SERVICES
Refractory goods, the following: 
Crucibles, moulds and pouring rods containing 97 per cent or more of
magnesium oxide or 97 per cent or more of beryllium oxide or 85 per
cent or more of zirconium oxide.
Thorium and its compounds and mixtures containing such substances. 
Uranium and its compounds and mixtures containing such substances.
Valves, with bellows seal, wholly made of or lined with aluminium, nickel or alloy
containing 60 per cent or more of nickel.
Group 3 
Electrical, Electronic and Scientific Appliances
A. Amplifiers the following: 
Amplifiers designed to operate at frequencies in excess of 300
megacycles per second.
Amplifiers, tuned, having a bandwidth which exceeds 10 megacycles
per second or 10 per cent of the mean frequency, whichever is less,
Amplifiers, untuned, having a bandwidth which exceeds 10 megacycles
per second.
Amplifiers, direct current, having a noise level (referred to the input
circuit) of 10- 16  watts or less, or a zero drift in one hour corresponding
to a change in input power of 10- 16  watts or less, or both these
characteristics.
In this entry - 
"bandwidth" means the band of frequencies over which the power amplification
does not drop to less than one-half of its maximum value; and
"mean frequency" means the arithmetic mean between the frequencies at which
the power amplification is one-half of its maximum value,
Apparatus for automatically sorting electronic components in respect of their
electrical characteristics.
Apparatus designed to jam or otherwise interfere with radio reception, and parts
specially designed therefor.
Apparatus of a kind used for detecting or locating objects under water by
magnetic, acoustic or ultrasonic methods, except marine depth sounders of a kind
used solely for measuring the depth of water or the distance of submerged objects
vertically below the apparatus; specialized components of such apparatus.
Capacitors, tantalum electrolytic.
Centrifugal testing apparatus possessing any of the following characteristics:
( a ) driven by a motor or motors having a total rated horse power greater
than 400 horse power;
( b ) capable of carrying a load of 250 pounds or more;
( c ) capable of exerting a centrifugal acceleration of 8 g or more on a load of
200 pounds or more.
Communication and detection equipment of a kind using infrared radiation or
ultrasonic waves, and specialized parts therefor.
CONTROL OF RE-EXPORTS OF SUPPLIES AND SERVICES [ S.L.117.06 5
Communication equipment employing tropospheric, ionospheric or meteoric
scatter phenomena and specially designed sub-assemblies, parts and test equipment
therefor.
Communication, navigation, direction finding and radar equipment, the
following- 
(1) Airborne communication equipment and specialized parts and components
therefor.
(2) Airborne navigation equipment and direction finding equipment, the
following -
( a ) Altimeters, pulse modulated.
( b ) Equipment designed to make use of the Doppler frequency phenomena.
( c ) Equipment utilizing the constant velocity or the rectilinear propagation
characteristics of electromagnetic waves having frequency less than 4 x
10 14  cycles per second (0.75 microns), or both.
( d ) Equipment, direction finding, operating at frequencies greater than 5
megacycles per second.
(3) Airborne radar equipment.
(4) Ground and marine radar equipment, the following -
( a ) Radar equipment, other than commercial equipment designed for pulse
operation at frequencies between 1,300 megacycles per second and
1,660 megacycles per second, 2,700 megacycles per second and 3,900
megacycles per second, or 8,500 megacycles per second and 10,000
megacycles per second, and having-
(i) in the case of marine navigation radar, a peak output power to the
aerial system of 75 kilowatts or less, and
(ii) in the case of ground based radar, a peak output power to the
aerial system of less than 50 kilowatts and a maximum usable
range against the largest airborne target of less than 50 nautical
miles.
( b ) Radar equipment incorporating -
(i) permanent echo cancellation facilities, or
(iii) aerials with circular polarization.
( c ) Radar equipment utilizing other than conventional pulse modulation and
signal processing techniques.
( d ) Ground direction finding equipment operating at frequencies greater
than 5 megacycles per second.
(5) Ground and marine equipment for use with airborne navigation equipment
utilizing the constant velocity or the rectilinear propagation characteristics of
electromagnetic waves having frequency less than 4 x 10 14  cycles per second (0.75
microns), or both.
(6) Specialized parts, specialized accessories and specialized testing or
calibrating equipment for use with apparatus mentioned in headings (2), (3), (4) or
(5) of this entry.
Compasses and gyroscopic apparatus, the following:
( a ) Automatic pilots, except marine types for surface vessels.
6 [ S.L.117.06 CONTROL OF RE-EXPORTS OF SUPPLIES AND SERVICES
( b ) Gyro compasses, North-seeking only, possessing one or more of the
following characteristics:
(1) automatic correction for the effects on compass accuracy of changes in
ship’s speed, acceleration, or latitude;
(2) provision for accepting ship’s data as an electrical input;
(3) provision for setting in corrections for current set and drift;
(4) utilization of accelerometer, rate gyro, rate integrating gyros or
electrolytic levels as sensing devices;
(5) provision far determining and electrically transmitting ship’s level
reference data (roll, pitch) in addition to own ship’s course data.
( c ) Gyro-magnetic compasses.
( d ) Gyro-stabilisers other than the kinds used for stabilising an entire surface
vessel.
( e ) Gyroscopes, high precision or miniaturised, designed for use in ship inertia
navigation system or in the guidance systems of weapons and aircraft. 
( f ) Pressure proof ship’s course indicators.
( g ) Transmitting magnetic compasses specially designed for submarines. 
( h ) Specially designed parts and components for any of the foregoing.
B. Components, electronic, capable of reliable performance in relation to their
electrical and mechanical characteristics and maintaining their design service life-
time while operating - 
( aa ) over the whole range of ambient temperatures extending from below -45º
Centigrade to above 100º Centigrade, or
( bb ) at ambient temperatures of 200º Centigrade or higher.
Computers, electronic, other than business type machines, accounting machines
and statistical calculating machines.
Control equipment, the following - 
( a ) Synchros, the following - 
(1) Control types (transmitters, differential transmitters and transformers)
rated to have an electrical error of 18 minutes or less when tested by the
proportional voltage method. 
(2) Torque types - 
(i) Transmitters and differential transmitters rated to have an
electrical error of 18 minutes or less when tested by the
proportional voltage method. 
(ii) Receivers and differential receivers rated to have an accuracy of
1.5 degrees or less when tested by the dynamic method.
( b ) Resolvers, including single-phase/single-phase, single-phase/two-phase,
two-phase/two-phase, and three phase/two-phase types -
(1) with a rated electrical error 0.5 degrees or less, or
(2) with a rated perpendicularity error between axes of 10 minutes or less;
or
(3) with a rated null voltage of 10 millivolts or less per maximum volt
output.
CONTROL OF RE-EXPORTS OF SUPPLIES AND SERVICES [ S.L.117.06 7
( cc ) Amplifiers, electronic or magnetic, designed for use with resolvers, the
following -
(1) Isolation types. 
(2) Summing types.
( dd ) Linear induction potentionmeters -
(1) with a rated linearity of one per cent or less, or
(2) with a rated null voltage of 10 millivolts or less per maximum volt output.
( ee ) Induction rate generators - 
(1) with a rated linearity of one per cent or less, or
(2) with a rated signal-to-noise ratio of 50 to 1 or greater, or temperature-
compensated or temperature-corrected.
( ff ) Servo motors (gear-head or plain)
(1) designed to operate from power sources of more than 300 cycles per
second, or 
(2) designed to have a torque-to-inertia ratio of 3,500 radians per second or
greater.
( gg ) Potentiometers, the following:
(1) Linear potentiometers with a rated linearity of 0.1 per cent or less 
(2) Non-linear potentiometers with a rated conformity of one per cent or
less.
Crystal signal diodes (excluding photodiodes), the following:
Point contact type diodes suitable for use at frequencies higher than
300 megacycles per second.
Junction type diodes in which the basic semiconductor material is
other than germanium. 
Junction type diodes in which the basic semiconductor material is
germanium, and which are suitable for use at frequencies higher than
50 megacycles per second. 
Specially designed parts for any of the foregoing.
C. Electric generators, mobile types, with a maximum continuous rating of
more than 5,000 kilowatts.
Electric-impulse generators of a kind used for providing recurring impulses of
peak power exceeding 150 kilowatts or of a duration of less than 0.1 microsecond;
pulse transformer and pulse forming equipment and delay lines being parts specially
designed for such electric-impulse generators.
Electromagnetic waveguides and components therefor, the following:
Ferrite waveguide components for use at all frequencies.
Rigid waveguides for use of frequencies in excess of 12,500 megacycles
per second. 
Flexible waveguides of all types.
Electronic and precision instruments and apparatus, the following - 
( a ) Electronic instruments, the following - 
8 [ S.L.117.06 CONTROL OF RE-EXPORTS OF SUPPLIES AND SERVICES
(1) Frequency measuring equipment and frequency standards with an
accuracy better than 0.00001 per cent
(2) Instruments operating at frequencies exceeding 300 megacycles per
second.
( b ) Oscilloscopes (cathode ray) and specialized parts therefor, the following: 
(1) Oscilloscopes possessing any of the following characteristics -
(i) a bandwidth greater than 12 megacycles per second;
(ii) a time base shorter than 0.04 microseconds per centimetre;
(iii) containing or designed for -
( a ) the use of one or more cathode ray tubes having three or more
electron guns, or
( b ) three or more cathode ray tubes; 
(iv) employing accelerating potentials in excess of 5,000 volts. 
(2) Specialized parts and accessories, the following:
Amplifiers and pre-amplifiers having a bandwidth greater than 12
megacycles per second.
In this entry "bandwidth" means the band of frequencies over which the deflection
on the cathode ray tube does not fall below 70.7 per cent of that at the maximum
point, measured with a constant input voltage to the amplifier.
D. Electronic vacuum tubes or valves, the following -
( a ) (1) Cathode ray tubes specially designed or of a kind used for radar
equipment described in the entry in this Group relating to
communication, navigation, direction finding and radar equipment.
(2) Cathode ray tubes with writing speeds of more than 3,000 kilometres per
second, or with three or more electron guns. 
( b ) (1) Thyratron and modulator gas-discharge tubes rated for continuous
operation with peak current and peak voltage exceeding 100 amperes
and 9,000 volts at a pulse repetition frequency of 200 or more pulses per
second.
(2) Hydrogen thyratron tubes, of any rating.
( c ) Valves whose output-input ratio at 300 megacycles per second is 50 per
cent or more of the output-input ratio at 20 megacycles per second when
measured under the same operating voltages and load impedance.
( d ) Valves of a kind specially designed for use at frequencies of more than
300 megacycles per second
( e ) Indirectly heated valves of a kind that can be passed through a circular
hole 7.2 millimetres in diameter. 
( f ) Valves designed to withstand - 
(i) sinusoidal vibration of greater than 2g for continuous periods in excess
of 20 hours at frequencies between 25 and 170 cycles per second, or 
(ii) acceleration of short duration (shock) greater than 1,000g.
( g ) Valves constructed with a ceramic envelope.
( h ) Valves designed for operation in ambient temperatures exceeding 100º
Centigrade.
CONTROL OF RE-EXPORTS OF SUPPLIES AND SERVICES [ S.L.117.06 9
( i ) Amplifier klystrons.
( j ) Travelling wave tubes.
( k ) Image converters and electronic storage tubes including memory
transformers of radar pictures and ruggedized photo-conductive-type
tubes (excluding commercial standard television broadcasting camera
tubes and commercial standard X-ray amplifier tubes).
( l ) X-ray tubes, flash discharge types.
E. Equipment designed to provide secrecy facilities on either voice or
telegraph, line or radio communication circuits other than those systems making use
at frequency inversions or band scrambling techniques.
Ion microscopes having a resolving power better than 10 angströms.
Line communication transmission equipment, the following - 
Terminal and intermediate repeater or amplifier equipment designed to
deliver, carry or receive frequencies higher than 16 kilocycles per
second into, or in, a line communication system.
Multi-channel telegraph terminal transmitting and receiving equipment. 
Specialized components, accessories, and sub-assemblies for the above
equipment.
Magnetic recorders or reproducers (other than those designed for voice or music)
and parts and recording media specially designed therefor.
Magnetometers of the following types - 
fluxgate;
electron beam sensing; 
paramagnetic; 
nucleonic;
and parts specially designed therefor.
Materials designed and manufactured for use as absorbers of electromagnetic
waves having frequencies greater than 2 x 10 8  cycles per second and less than 3 x
10 12  cycles per second.
Measuring and counting apparatus, the following:
( a ) Time interval measuring equipment with self-contained reference frequency,
having one or both of the following characteristics -
(1) capable of measuring time intervals of 0.1 second or less with an error
not exceeding one microsecond plus 0.001 per cent of the interval
measured;
(2) incorporating counting circuits capable of counting at rates in excess of
one megacycle per second.
( b ) Counting equipment capable of counting at rates in excess of one megacycle
per second:
F. Photo-electric cells, the following -
Photo-electric cells, photo-conductive cells (including photo-transistors
and similar cells) with a peak sensitivity at a wavelength longer than
12,000 angströms.
Photo-transistors (photo-conductive cells including photo-diodes) with
10 [ S.L.117.06 CONTROL OF RE-EXPORTS OF SUPPLIES AND SERVICES
response time constant of one millisecond or less measured at the
operating temperature of the cell for which the time constant reaches a
minimum.
G. Photographic apparatus, the following: 
(1) High speed cameras capable of recording at rates in excess of 250,000
frames per second.
(2) High speed cinematograph cameras, the following:
( a ) Cinematograph cameras employing film of a width of 35 millimetres or
less, capable of recording at rates in excess of 3,000 frames per second
using as the lighting source a steady light flow.
( b ) Cinematograph cameras employing film of a width of 35 millimetres or
less, capable of recording at rates in excess of 10,000 frames per second
using as the lighting source flash apparatus connected to the unwinding
system.
( c ) Cinematograph cameras employing film wider than 35 millimetres and
capable of recording at rates exceeding 64 frames per second.
(3) Photographic microflash apparatus capable of giving a flash of 10
microseconds or shorter duration at a minimum recurrent frequency of 200 flashes
per second.
Photomultiplier tubes, the following - 
Photomultiplier tubes with all the following characteristics for a colour
temperature of 2,850 degrees Kelvin: 
(i) sensitivity exceeding the figure of 60 microamperes per lumen;
(ii) overall gain for a mean output current of one milliampere
exceeding 10 8;
(iii) dark current plus noise less than 5x10- 16  ampere mean per square
centimetre of active cathode surface.
Photomultiplier tubes of all types for which the maximum sensitivity
occurs at wavelengths longer than 7,500 angtroms.
Piezo-electric quartz crystals, blanks, plates, bars, rods and toroids, worked or
unworked, mounted or unmounted.
H. Radio receivers, panoramic, being receivers which search automatically a
part of the radio frequency spectrum and indicate the signals received, and parts
specially designed for such receivers.
Radio relay communications equipment other than short range and low power
links for transmissions between camera or studio and the television transmitter;
specialized components and sub-assemblies therefor.
Radio spectrum analysers, being apparatus capable of indicating the single-
frequency components of multi-frequency oscillations, designed to operate at
frequencies in excess of 300 megacycles per second; parts specially designed
therefor.
Radio transmitters and components, the following: 
( a )  Transmitters or transmitter amplifiers designed to operate:
(1) at output carrier frequencies between 108 and 156 megacycles per
second, or 
CONTROL OF RE-EXPORTS OF SUPPLIES AND SERVICES [ S.L.117.06 11
(2) at output carrier frequencies greater than 223 megacycles per second
other than television broadcasting transmitters and amplifiers therefor
operating between 470 band 585 megacycles per second or between 610
and 940 megacycles per second.
( b ) Transmitters or transmitter amplifiers designed to provide any of the
following features: 
(1) any system of pulse modulation other than amplitude, frequency or
pulse modulated television;
(2) special facilities to give continuous operation (on any carrier frequency
outside the internationally agreed broadcasting hands) in inter
connection with land-line telephone circuits or switchboards, such as
voice operated gain-adjusting circuits, automatic volume compression
and expansion circuits, and automatic monitoring;
(3) rapid selection of more than 20 channels;
(4) operation over a range of ambient temperatures extending from below -
45º Centigrade to about 75º Centigrade;
(5) facilities providing a multiplicity of alternative output carrier
frequencies controlled by a lesser number of piezo-electric crystals and
not forming multiples of a common control frequency;
( c ) Components and sub-assemblies, including modulators and modulation
amplifiers, specially designed for use in any such transmitters.
I. Telegraph apparatus designed for the transmission or reception of messages
at a speed exceeding 200 words per minute or 150 bauds, whichever is the less,
except equipment operating at a speed of 300 bauds where the corresponding number
of words does not exceed 65 words per minute; parts and accessories specially
designed therefor.
Transistors and related devices (or related semi-conductor amplifying devices
such as fieldistors, spacistors and technetrons) -
( a ) of any type using a basic semi-conductor material other than germanium, 
( b ) having any of the following characteristics - 
(1) designed to be capable of operation at alpha cut-off frequencies greater
than 20 megacycles per second;
(2) designed to have a collector dissipation in excess of 100 milliwatts at
alpha cut-off frequencies greater than 500 kilocycles per second; 
(3) designed to operate with collector voltages greater than 40 volts; 
(4) designed to operate with mean collector currents greater than 3
amperes;
specialized parts for any of the foregoing. 
Group 4
Chemicals
Ammonium perchlorate. 
Beryllium compounds.
Boron compounds, and mixtures, the following: 
( a ) Boric acids and the esters and ammonium, calcium, magnesium, potassium
and sodium salts of boric acids, but not including perborates.
12 [ S.L.117.06 CONTROL OF RE-EXPORTS OF SUPPLIES AND SERVICES
( b ) Boric oxide. 
( c ) Boron carbide. 
( d ) Boron nitride. 
( e ) Boron trichloride and its complexes. 
( f ) Boron trifluoride and its complexes. 
( g ) Fluoroborates.
( h ) Other boron compounds and mixtures containing an aggregate of 10 per cent
or more of boron, whether in combined or elemental forms, but excluding -
Metal borates other than those specified in heading ( a ) of this entry.
Perborates.
Cellulose nitrate (nitrocellulose).
Chlorine trifluoride. 
mono Chlorodifluoromethane.
Chlorotrifluoroethylene.
Cobalt compounds having a cobalt content equivalent to 30 per cent, or more in
the anhydrous material (other than paint driers, cobalt, organic artificial colouring
matters and other paint pigments).
Dichlorotetrafluoroethane. 
sym Diethylsymdiphenylurea (carbamite or centralite). 
Diethylenetriamine.
sym Dimethy sym diphenylurea (carbamite or centralite). 
asym Dimethylhydrazine.
Dinitrophenol. 
Diphenylamine. 
asym Diphenylurea. 
Ethyl diphenylcarbamate (diphenylurethane). 
Ethyl asym diphenylurea.
Ethyl dl-o-tolylcarbamate (di- o -tolylurethane). 
Ethyl  N -ethylphenylcarbamate (ethylphenylurethane).
Fluorine.
Guanidine nitrate. 
Hydrazine.
Hydrazine hydrate.
Hydrazine nitrate.
Hydrogen peroxide containing 50 per cent or more of hydrogen peroxide: 
Lead azide.
Lead styphnate (lead trinitroresorcinoxide). 
Lead thiocyanate. 
CONTROL OF RE-EXPORTS OF SUPPLIES AND SERVICES [ S.L.117.06 13
Lithium compounds.
Magnesium oxide of a purity of 97 per cent or more. 
Methyl asy mdiphenylurea.
Molybdenum disulphide of a purity of 86 per cent or more. 
Nitric acid, fuming.
2-Nitrodiphenylamine. 
Nitromethylaniline.
Pentaerythritol tetranitrate. 
Picrates.
Picric acid. 
Sodium azide. 
Tantalum compounds.
Tetrafluoroethylene. 
Trichlorotrifluoroethane. 
Zirconium compounds in which the ratio of hafnium content to zirconium content
is less than one part to 500 parts by weight.
Zirconium oxide thermally stabilized with calcium oxide or magnesium oxide or
both.
Group 5 
Minerals and Metals
In this Group - 
"raw materials" means ores, concentrates, matte, regulus, residues and dross
(ashes), from which the metal described in the entry can be extracted; 
"crude forms" means anodes, balls, bars (including notched bars and wire bars),
billets, blocks, blooms, briquettes, cathodes, cakes, crystals, cubes, dice, grains,
granules, ingots, lumps, pellets, pigs, powder, rondelles, shot, slabs, slugs, sponge
and sticks;
"semi-fabricated forms" means the following (whether or not coated, plated,
drilled or punched) -
(1) wrought or worked materials, fabricated by rolling, drawing, extruding,
forging, impact extruding, pressing, graining, atomising and grinding, the
following-
angles, channels, circles, discs, dust, flakes, foil and leaf, forgings,
plates, powder, pressings and stampings, ribbons, rings, rods (including
bare welding rods, wire rods and rolled wire), sections, shapes, sheets,
strip, pipes and tubes (including tube rounds, squares and hollows) and
drawn or extruded wire; or
(2) cast material produced by casting in dies, sand, metal, plaster or other types
of moulds, including high pressure castings, sintered forms and forms made by
powder metallurgy.
Beryllium, the following -
Ores (other than gem grade beryl) and concentrates.
14 [ S.L.117.06 CONTROL OF RE-EXPORTS OF SUPPLIES AND SERVICES
Beryllium and alloys containing more than 50 per cent of beryllium, in crude
or semi-fabricated forms other than windows for medical X-ray machines).
Boron, the following:
Boron minerals, crude and refined.
Ferro-boron, whether briquetted or not.
Boron and alloys containing 10 per cent or more of boron, in crude or semi-
fabricated forms.
Cobalt, the following -
Raw materials.
Ferro-cobalt, whether briquetted or not.
Cobalt and alloys containing -
( a ) 50 per cent or more of cobalt, or
( b ) 9 per cent or more of cobalt together with 14 per cent or more of
chromium, 
in crude or semi-fabricated forms, or scrap.
Germanium of a resistivity of 50 ohms per centimetre or more, in crude or
semifabricated forms.
Iron and steel, the following - 
Iron, steel and alloys of iron or steel, being iron, steel and alloys containing 50 per
cent or more of iron if -
( a ) (i) armour plate
(ii) precipitation hardening steels containing 4 per cent or more of
nickel; or
( b ) containing one or more of the following constituents in the
proportions stated: 
(i) 10 per cent or more of molybdenum;
(ii) 5 per cent or more of molybdenum together with more than 14 per
cent of chromium;
(iii) 6 per cent or more of cobalt, except permanent magnetic metals
with a cobalt content of 25 per cent or less; 
(iv) 1.5 per cent or more of niobium (columbium) or tantalum or both;
(v) 32 per cent or more of nickel;
(vi) 32 per cent or more of alloying element (other than iron) one of
which is nickel, together with 0.4 per cent or more of titanium,
niobium (columbium) or tantalum, 
in crude or semi-fabricated forms.
Lithium, the following -
Raw materials.
Lithium in crude or semi-fabricated forms.
Magnesium alloys containing 50 per cent or more of magnesium and one or more
of the following constituents in the proportions stated:
( a ) 0.4 per cent or more of zirconium;
( b ) 1.5 per cent or more of thorium;
CONTROL OF RE-EXPORTS OF SUPPLIES AND SERVICES [ S.L.117.06 15
( c ) 1.0 per cent or more of rare earth metals (cerium mischmetall),
in crude or semi-fabricated forms, or scrap.
Magnetic materials in all forms (including specialized forms such as core
assemblies, laminations, tapes and wound cores), having any of the following
characteristics:
(1) thickness of 0.0004 inch or less;
(2) initial permeability 50,000 or over;
(3) remanence 98 per cent or over of maximum flux for materials having
magnetic permeability;
(4) a composition capable of an energy product greater than 6 mega-
gaussoersteds, or containing more than 25 per cent of cobalt;
(5) in the case of silicon steels, a core loss of 0.45 watt per pound or less
measured at a flux density of 13,000 gauss and a frequency of 50 cycles
per second. 
Minerals, raw and treated (including residues and tailings), containing more than
0.05 per cent of uranium or thorium, singly or together, including but not limited to,
the following -
Monazite and monazite sands.
Ores containing thorium including uranothorianite. 
Ores containing uranium including pitchblende. 
Molybdenum, the following - 
Ferro-molybdenum, whether briquetted or not.
Molybdenum and alloys containing 60 per cent or more of molybdenum, in
crude or semi-fabricated forms (other than clean wire of a diameter not
exceeding 500 microns and which, after having been fully anxiealed, has an
elongation factor not exceeding 5 per cent for diameters up to 200 microns
and not exceeding 10 per cent for diameters of between 200 and 500
microns).
Molybdenum pipes and tubing, platinum clad.
Nickel, the following -
Raw materials.
Nickel powder.
Nickel-based alloys containing 32 per cent or more of nickel, in crude or
semi-fabricated forms.
Wire of a diameter of 0.1 millimetre or less containing 95 per cent or more
of nickel, and wire mesh, woven, composed of wire containing 95 per cent or
more of nickel and containing 60 or more wires per linear centimetre.
Niobium (columbium), the following:
Raw materials.
Ferro-niobium and ferro-niobium-tantalum, whether briqu-etted or not.
Niobium and alloys containing 60 per cent or more of niobium or 60 per cent
or more of niobium-tantalumin combination, in crude or semi-fabricated
forms, or scrap.
Platinum clad molybdenum pipes and tubing.
16 [ S.L.117.06 CONTROL OF RE-EXPORTS OF SUPPLIES AND SERVICES
Silicon of a purity of 99.9 per cent or more.
Tantalum, the following -
Raw materials.
Ferro-tantalum and ferro-tantalum-niobium (columbium), whether briquetted
or not:
Tantalum and alloys containing 60 per cent or more of tantalum or 60 per
cent or more of tantalum-niobium (columbium) in combination, in crude or
semi-fabricated forms; or scrap.
Thorium and alloys containing 1.5 per cent or more of thorium, in crude or semi-
fabricated forms.
Titanium and alloys containing 70 per cent or more of titanium, in crude or semi-
fabricated forms, or scrap.
Tungsten wire and filament, the following -
(1) Wire, coated or covered.
(2)  Wire, not coated or covered, other than wire of a diameter less than 600
microns the tensile strength of which is not more than 35 grammes per
milligram (140 kilogrammes per square millimetre) when measured on
the wire drawn down to 180 microns or less and heated in a hydrogen
atmosphere of 2,100º Centigrade for a period of 10 minutes.
(3) Cut coils, coated or covered.
(4) Cut coils, not coated or covered, other than -
( a ) coiled coil filaments;
( b ) single coil lamp filaments having any of the following
characteristics -
(i) set or sintered;
(ii) a diameter of 19 microns or less;
(iii) a diameter of 250 microns or more and a length not exceeding
100 millimetres.
Uranium, the following -
Ferro-uranium, whether briquetted or not;
Uranium and alloys containing any percentage of uranium, in crude or semi-
fabricated forms.
Zirconium, in which the ratio of hafnium content to zirconium content is less than
one part to 500 parts by weight, the following:
Ferro-zirconium, whether briquetted or not.
Zirconium and alloys containing more than 50 per cent of zirconium in crude
or semi-fabricated forms.
Manufactures wholly of zirconium or of alloys containing more than 50 per
cent of zirconium.
Group 6
Engineering products
A. In this Group - 
"a specified corrosion-resistant material" means polytetrafluofaefhylene,
CONTROL OF RE-EXPORTS OF SUPPLIES AND SERVICES [ S.L.117.06 17
polychlorotrifluoroethylene or metals or alloys containing - 
(i) 90 per cent or more of tantalum, titanium or zirconium, either separately
or combined, or
(ii) 50 per cent or more of cobalt or molybdenum, either separately or
combined.
Ball or roller bearings, and parts thereof, the following:
( a ) Ball or cylindrical roller bearings (other than separable (magneto type), ball
bearings and ball thrust bearings) manufactured to tolerances specified in Part II of
this Schedule or closer, and possessing one or more of the following characteristics: 
(1) made of any material other than -
(i) low carbon steel containing not more than 0.4 per cent of carbon and no
other elements except those present as impurities or in such low
quantities as not to modify the basic characteristics of the steel;
(ii) high carbon chromium steel type En 31 as specified in British Standard
970: 1955 (wrought steels), or equivalent types normally used in the
manufacture of ball or roller bearings; 
(iii) nickel-molybdenum steel type En 34 as specified in British Standard
970: 1955 (wrought steels), or equivalent types normally used in the
manufacture of ball or roller bearings;
(2) processed by heat treatment for the purpose of stabilizing them for use at
normal operation temperatures over 150º. Centigrade;
(3) having special low torque or quiet running performance beyond that
required for industrial purposes, to provide a superior operating performance for
military purposes;
(4) specially designed for use in military equipment and differing substantially
in design from normal bearings in order to provide a superior operating performance.
( b ) Tapered roller, spherical roller and thrust roller bearings having an inner
ring bore diameter measuring more than 400 millimetres (15.75 inches).
( c ) Parts of ball or roller bearings, the following -
Outer rings, inner rings, retainers, balls, rollers and sub-assemblies
usable only for bearings described in heads ( a ) or ( b ) of this entry.
B. Cables, the following - 
Coaxial-type cables (including submarine types) designed for
telecommunication and radar purposes other than those of a type designed or
in common use for domestic radio and television receivers. 
Communication cable (including submarine cable) containing more than one
pair of conductors and containing any conductor, single or stranded,
exceeding 0.9 millimetre in diameter.
Centrifugal counter-current solvent extractors specially designed for the
extraction of radio-active substances.
Compressors and blowers, multistage, with an overall compression ratio of 2:1 or
more coupled with a capacity of over 372,000 cubic feet per minute, or an overall
compression ratio of 3:1 or more coupled with a capacity of over 106,000 cubic feet
per minute.
Containers, jacketted, including mobile units, of 500 gallons capacity or over,
18 [ S.L.117.06 CONTROL OF RE-EXPORTS OF SUPPLIES AND SERVICES
designed for the storage or transportation of the following liquefied gases: 
Argon.
Helium.
Hydrogen. 
Nitrogen. 
Oxygen. 
Ozone.
Equipment for the production or concentration of deuterium oxide.
Equipment specially designed for the conversion of  di nitrogen tetroxide to nitric
acid of 98 per cent or higher concentration or for the concentration of  di nitrogen
tetroxide or nitric oxides or mixtures thereof.
Equipment specially designed for the purification and processing of germanium,
other than equipment for zone purification.
Equipment specially designed for the purification and processing of silicon. 
Furnaces, electric, specially designed for the recovery of titanium or zirconium
from scrap.
Gas liquefying equipment, the following:
Equipment for the separation of helium from natural gases.
Equipment specially designed for the production of gases in liquid form,
capable of operating at pressures of 300 pounds per square inch gauge and
over and producing one ton or more per day of gas in liquid form, other than: 
( a ) Plants not capable of producing more than 25 per cent of their total
daily product as extractable gas in liquid form.
( b ) Plants specially designed for liquefying chlorine and ammonia. 
( c ) Stationary equipment for liquefying carbon dioxide.
( d ) Equipment for liquefying low molecular weight refinery gases. 
Liquid fluorine producing equipment.
C. Machines and apparatus for the manufacture and testing of electronic valves,
the following: 
Machines and apparatus specially designed for the manufacture and testing of
electronic valves, transistors and crystal diodes (including components and
sub-assemblies therefor) described in Group 3.
Machines and apparatus specially designed for the automatic or semi-
automatic assembly or testing of electronic valves, transistors and crystal
diodes (including components and sub-assemblies therefor).
Machines and apparatus of the kind used for making telecommunication
cables, the following:
( a ) Machines of the kind specially designed for the manufacture of multi-
pair electric cables for telecommunication purposes, the following:
(1) Machines of the kind used for applying insulating material to
conductors.
(2) Machines of the kind used for laying conductors together or for
applying an insulating, separating, binding or identifying material
thereto. 
CONTROL OF RE-EXPORTS OF SUPPLIES AND SERVICES [ S.L.117.06 19
( b ) Machines of the kind specially designed for the manufacture of coaxial
electric cables, the following: 
(1) Machines of the kind used for applying insulating separators to
the inner conductor of air-spaced coaxial electric cables.
(2) Machines of the kind used for applying metal strip or sheet to
form the outer conductor of coaxial electric cables.
( c ) Machines of the kind used for laying up or stranding conductors, pairs,
quads, multiple units thereof, or coaxial tubes, to form complete cable
covers or parts thereof.
( d ) Automatic apparatus for controlling the diameter or the eccentricity of
extruded dielectric on wares and cables.
Machines, apparatus and tools specially designed for the manufacture and testing
of gas turbines, the following: 
Compressor case boring machines.
Compressor and turbine disc turning machines.
Machines and apparatus for making or measuring gas turbine blades.
Rotor grinding machines.
Surface broaching tools for the manufacture of gas turbine blades and discs. 
Machines, milling, having a travelling head or heads, capable of milling aircraft
spars.
Machines for milling aircraft skin.
Machines, metalworking, the following: 
Deep hole drilling machines of the kind designed to use tubular drills or bars in
which the coolant passes through the drill or bar.
D.  Forging hammers, the following -
Gravity hammers having a falling weight of over 10 tons.
Steam, air of mechanical hammers (except counter-blow hammers) of rated
size over 10 tons.
Counter-blow hammers of rated size of 180,825 foot pounds or more. 
Horizontal impact hammers, hydraulically actuated, of rated size of 10,000
foot pounds or more.
Gear-making or gear finishing machinery, the following -
Gear-grinding machines, generating type, of 36 inches work diameter or
over. 
Machines capable of the production of gears having a pitch finer than 0.5
module.
Grinding machines, the following -
Internal grinding machines of the kinds incorporating or specially designed
for the utilization of grinding heads designed or rated for operation at speeds
in excess of 80,000 revolutions per minute.
Jig grinding machines with any traversing motion (longitudinal, transverse
or vertical) exceeding 44 inches. 
Jig boring machines with any traversing motion (longitudinal, transverse or
vertical) exceeding 44 inches.
20 [ S.L.117.06 CONTROL OF RE-EXPORTS OF SUPPLIES AND SERVICES
Machines incorporating electronic closed loop feed back controls in which a
continuous feed back of information from the work piece or tool or work piece
carrier or tool-holder itself results in continuous correction of the control commands.
Presses hydraulic and mechanical, with total rated pressures of ever 5,000
tons.
Spinning lathes designed for use with or equipped with spindle drive motor
exceeding 25 horse power.
Machines specially designed for the working or forming of aircraft sheet, aircraft
plate or aircraft extrusions. 
Machine tool parts, accessories and associated apparatus, the following -
Electronic closed loop feed back controls for controlling machine tools in
which a continuous feed back of information from the work piece or tool or
work piece carrier or tool-holder itself results in continuous correction of the
control commands.
Grinding heads and spindle assemblies for internal grinding machines, designed or
rated for operation at speeds in excess of 80,000 revolutions per minute. 
Marine steam boilers designed to operate at temperatures of 593º Centigrade and
above.
Metal cutting and working tools for machine operations, the following -
Deep hole drills or bars of the type in which a hardened steel or hard metal
cutting piece is fixed into a tubular shank and the coolant passes through the
drill or bar.
E. Pipe and tubing (metal) lined with polytetrafluoroethylene or
polychlorotrifluoroethylene.
Pipe valves, cocks and pressure regulators, either -
(1) designed to operate at temperatures below -130º Centigrade; or
(2) having all flow contact parts made of or lined with a specified corrosion
resistant material.
Plant for the production of military explosives and parts specially designed
therefor, including nitrators, continuous types.
Plant for the production of titanium metal (other than separate plant for the
production of titanium tetrachloride) and parts specially designed therefor.
Plant for the production of zirconium (other than separate plant for the production
of zirconium tetrachloride) and parts specially designed therefor.
Printed circuit equipment, the following - 
Equipment specially designed to produce electronic assemblies -
( a ) by depositing or printing on insulating panels, including plates or
wafers, or otherwise forming  in situ , component parts other than basic
wiring, or
( b ) by automatically inserting or soldering components on insulating
panels, including plates or wafers, to which wiring is applied by
printing or other means.
F. Pumps (other than vacuum pumps) capable of delivering liquids separately
or in combination with solids, gases, or solids and gases, and having any of the
following characteristics - 
CONTROL OF RE-EXPORTS OF SUPPLIES AND SERVICES [ S.L.117.06 21
(1) designed to move molten metals by electromagnetic forces; 
(2) designed to operate at temperatures below -130º Centigrade;
(3) all flow contact surfaces made of a specified corrosion-resistant,
material. 
Rock drill bits rotary type, that is to say, of a kind having cones or sections which
rotate separately and independently of the rotation of the body of the bit. 
Rolling mills; the following: 
( a ) having the work-rolls supported by multiple back-up rolls or bearings;
( b ) having multiple work-rolls rotating in a planetary form around the back
up rolls;
( c ) continuous cold strip mills, more than 3-high.
Group 7 
Transport Equipment
Compression ignition (diesel) engines capable of developing 50 brake horse power
and over and having a non-magnetic-content exceeding 50 per cent of their total
weight.
Construction equipment built to military specifications, specially designed for
airborne transportation.
Mechanically propelled vehicles, tractors and lift trucks, possessing or built to
current military specifications differing materially from normal civilian
specifications.
Group 8
Miscellaneous
Alkyl, polysulphide liquid polymers (other than water dispersions).
Condenser tissue, that is, synthetic film for dielectric use, of 0.0015 inch (0.038
millimetre) or less thickness.
Fluorinated silicone rubbers and other flourinated elastomeric materials, and such
organic intermediates for their manufacture as contain 10 per cent or more of
combined fluorine.
Fuels for aircraft turbine engines, the following -
( a ) wide cut gasoline types;
( b ) kerosene types having a freezing point below -60º Centigrade;
( c ) high flash kerosene types having a minimum flash point of 60º
Centigrade;
( d ) any liquid fuel, including petroleum, which contains high energy
components or compounds thereof, having a gross calorific value of not
less than 23,400 British Thermal Units per pound.
High octane blending agents for aircraft fuels, the following -
( a ) Alkylates, aviation grade.
( b ) Isopentane. 
( c ) Neohexane.
22 [ S.L.117.06 CONTROL OF RE-EXPORTS OF SUPPLIES AND SERVICES
Hydraulic fluids, the following: 
( a ) petroleum based, having a kinematic viscosity of 4.6 centistokes or
greater at 98.9º Centigrade and a pour point of -34.4º Centigrade or
lower and a viscosity index of 130 or higher;
( b ) synthetic, having a viscosity of not more than 4,000 centistokes at -54º
Centigrade and not less than 1.5 centistokes at 150º Centigrade. 
Lubricating oils and greases, synthetic (ester type) being or containing -
(1) esters of dibasic saturated aliphatic acids combined with one or both of the
following - 
( a ) saturated aliphatic monohydric alcohols, where both of the two
constituents contain six or more carbon atoms, and
( b ) polyglycols where one or both of the two constituents contain six or
more carbon atoms; or 
(2) fluoro-alcohol esters;
other than oils and greases containing either -
( a ) 50 per cent or more of neutral castor oil, or
( b ) 5 per cent or more of neutral castor oil and 50 per cent or more of castor
oils and petroleum oil together.
Polychlorotrifluoroethylene and manufactures wholly thereof. 
Polytetrafluoroethylene and manufactures wholly thereof. 
Silicone fluids and greases, the following - 
Halogenated silicone fluids. 
Lubricating greases capable of operating at temperatures of 180º Centigrade
or higher and having a drop point of 220º Centigrade or higher.
PART II
Ball and roller bearings: tolerances for bore and outside diameter, parallelism 
of races and wobble (parallelism of track to faces) referred to in Group 6 of 
Part I of this Schedule.
1. INNER RING
Bore Sizes
Inch Type
Over 0 
including 
2 in.
Over 2 
including 
3 in.
Over 3 
including 
5 in.
Over 5 
including 7 
in.
Over 7 
including 10 
in.
Over 10 in.
Metric Type
Over 0 
including 
50 mm.
Over 50 
including 
80 mm.
Over 80 
including 
120 mm.
Over 120 
including 
180 mm.
Over 180 
including 
250 mm.
Over 250 
mm.
Total bore 
tolerance (inches)  .0002 .0003 .0003 .0004 .0005 .0005
Eccentricity 
(inches) ................ .0002 .0002 .0003 .0003 .0004 .0005
Parallelism of 
races (inches) ....... .0002 .0002 .0003 .0003 .0004 .0005
Wobble or 
parallelism of track 
to faces (inches) ... .0003 .0003 .0004 .0004 .0005 .0006
CONTROL OF RE-EXPORTS OF SUPPLIES AND SERVICES [ S.L.117.06 23
2. OUTER RING
Outside Diameter Sizes
Inch Type Over 0 incl. 2 in. Over 2 incl. 3 in. Over 3 incl. 5 in. Over 5 incl. 6 in. Over 6 incl. 7 in.
Over 7 
incl. 10 
in.
Over 10 
incl. 12 
in.
Over 12 
incl. 16 
in.
Over 16 
in.
Metric 
Type
Over 0 
incl. 50 
mm.
Over 50 
incl. 80 
mm.
Over 80 
incl. 120 
mm.
Over 120 
incl. 150 
mm.
Over 150 
incl. 180 
mm.
Over 180 
incl. 250 
mm.
Over 250 
incl. 315 
mm.
Over 315 
incl. 
400mm
Over 400 
mm.
Total
outside
diameter
tolerance
(inches)  .0002 .0003 .0003 .0004 .0005 .0005 .0005 .0006 .0007
Eccentri-
city
(inches) .0002 .0003 .0004 .0004 .0005 .0005 .0006 .0007 .0008
Paralle-
lism of
races
(inches) .0002 .0002 .0003 .0003 .0003 .0004 .0005 .0005 .0006
Wobble or
paralle-
lism of
track to
faces
(inches) .0003 .0004 .0005 .0005 .0006 .0006 .0007 .0008 .0009
24 [ S.L.117.06 CONTROL OF RE-EXPORTS OF SUPPLIES AND SERVICES
Amended by: SECOND SCHEDULE
G.N. 389 of 1957.
Regulation (2)
Belgium
Bolivia
Canada
Congo
Denmark
France
Germany
Greece
Italy
Japan
Luxembourg
The Netherlands
Norway
Peru
The Philippines
Portugal
Ruanda Urundi
Turkey
United Kingdom
United States of America
CONTROL OF RE-EXPORTS OF SUPPLIES AND SERVICES [ S.L.117.06 25
THIRD SCHEDULE Substituted by:
L.N. 13 of 1961.
Albania
Bulgaria
China
Czech Republic
Hungary 
North Korea
North Viet Nam, that is, all that part of Viet Nam north of a line running from the
mouth of Song Ben Hat River along the course thereof to the village of Bo Ho Su
and thence due west to the frontier of Laos. *
Poland
Romania
Soviet Zone of Germany
Tibet
Ex-Union of Soviet Socialist Republics
*Note by the Law Commission:
These countries do not exist any more either legally or politically.
26 [ S.L.117.06 CONTROL OF RE-EXPORTS OF SUPPLIES AND SERVICES
FOURTH SCHEDULE
TRANSIT AUTHORISATION CERTIFICATE 
CERTIFICAT D’AUTORISATION DE TRANSIT
Country:
Pays :
Issuing Office:
Service d’emission
Number:
Numero :
1. It is certified that the goods listed below may be exported to
Il est certifie que le merchandises mentionees ci-après peuvent être
exportées a destionation de
(County of final destination -  Pays de destination finale )
(a) Commercial description of goods:
Designation commerciale des marchandises:
(b) Number of control-list:
Numero de la list de controle:
(c) Quantity of goods. Weight:
Quantité des marchandises. Poids:
Volume, Measurements, etc.:
Volume, Métrage, etc.:
(in words and in figures)
(en lettres et en chiffres)
(d) Value and terms of delivery:
Valeur et conditions de livraison:
(f.o.b., c.i.f., etc.)
(e) Number and date of issue of export licence:
Numero et date de la licence d’exportation:
(f) Any other remarks:
Observations eventuelles:
(*) Name and address of the exporter:
Nom et addresse de l’exporteur
At .............................., on:
À ................................, le:
Official stamp
Cachet
Signature:
(*) This section to be included in the form at the option of the country of export.
CONTROL OF RE-EXPORTS OF SUPPLIES AND SERVICES [ S.L.117.06 27
II. To be completed by the exporter or his representative before it is delivered
to Customs
A completer par l’exportateur on son représentant avant preséntation à la
douane.
(a) Number and type of packages or state if in bulk:
Numbre et expece des colis ou mention qu’il s’agit d’un envoi envrae ou
non emballe:
(b) Marks and numbers of packages: 
Numeros et marques des colis:
(if appropriate)
(s’il ya lieu)
(c)  Gross weight:
Poids brut:
Net weight:
Poids net:
(d) Means of transport:
Moyen de transport:
(e) Name and address of the carrier:
Nom et addresse du transporteur:
(Date)
Signature:
Exporter or his representative
L’exporteur or son representant.
III. To be completed by the Customs of the country of exportation
A complèter par la Douane du pays d’exportation
Customs reference No.
Declaration de sortie No.:
At ..................., on:
À  ...................., le:
Official stamp
Cachet Signature:
IV. A. To be completed by the Customs Office of exit in the first country of
transit.
Visa de la Douane de sortie du premier pays de transit.
Transhipment Entry No.
Declaration de transit no:
At ..................., on:
À ...................., le:
Official stamp
Cachet Signature:
B. To be completed by the Customs Office of exit in the second country of
transit.
Visa de la Douane de sortie du deuxième pays de transit.
Transhipment Entry No.
Declaration de transit no:
At ..................., on:
À ...................., le:
28 [ S.L.117.06 CONTROL OF RE-EXPORTS OF SUPPLIES AND SERVICES
Official stamp
Cachet
C. To be completed by the Customs Office of exit in the third country of
transit.
Visa de la Douane de sortie du deuxième pays de transit.
Official stamp
Cachet Signature:
NOTES
REMARQUES
(a) This Certificate is valid for four months from the date of the Customs stamp
in Part III.
Ce certificat est valable pendant quatre mois à partir de la date du visa
appose par la douane dans la cadre III.
(b) The customs authorities of the last transit country are requested to return
this certificate to the licensing authorities of their country.
Il est recommende aux autorités douanierés du dernier pays de transit de
renoyer le present certificat au service de licences de leru pays.
